I opened Fanucm here:
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And I got this, even though the dongle is indicated as inserted if MillCam Designer is opened. I had changed the parallel port BIOS to ECP type.
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Rechecking — Press ESC to abort




When I pressed Escape this error message turned up: Does it mean the RS232 Driver and others are not on the computer or something? If so, are they available somewhere?

Is this all that I am doing wrong?
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below is what I got when I ran drights[image: image4.png]=3
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