ELECTRICAL RECORD SHEET





DATE�
MACHINE TYPE�
SERIAL NUMBER�
CUSTOMER�
�
19/01/00�
CYCLONE�
90824A�
NORTHAMPTON COLLEGE�
�
Inspected by:








Address-DEPARTMENT OF ENGINEERING�
�
BOOTH LANE, NORTHAMPTON, NN3 3RF�
�
Cust order  n/o S012711�
�



Power requirements-				 		Transformer details(if supplied)


V-415�
Phase-3�
Hz-50�
V in-N/A�
V outN/A�
KVA-N/A�
�



Control system							    		 Software


 Control supplier                 Control type                 Control s/no	     	Denford-F    	    	  Denford-H	                Eprom	


FANUC�
21I - TA�
E996A0194�
C009E�
N/A�
�
�



Axis motors   	 Make	                   Model		  S/no		      Volts               Ac/Dc	    Phase


x-axis�
FANUC�
AO6B-0032-B075#7008�
�
176�
AC�
3�
�
y-axis�
�
�
�
�
�
�
�
z-axis�
FANUC�
AO6B-0032-B075#7008�
�
176�
AC�
3�
�
4th-axis�
N/A�
�
�
�
�
�
�



Axis drives		Make		                  Model			            S/no


x-axis�
FANUC�
AO6B-6093-H111�
EA9500530�
�
y-axis�
�
�
�
�
z-axis�
FANUC�
AO6B-6093-H111�
EA9500541�
�
4th-axis�
N/A�
�
�
�



Spindle motor


	 Make		      	Model		     S/no			     Volts	  Hz	     Ac/Dc	Phase


ABB�
4 KW�
�
420�
N/A�
AC�
3�
�



Spindle drive								  	      Spindle encoder(if fitted)


            Make	Model		   S/no		    Make		Model				  S/no


OMRON�
3G3FV�
E99240016026-045�
FANUC�
A680 - 0309 - T302�
�
�



Toolchanger									  	                       Invertor(if fitted)


     Make		Model	       S/no	     Stations    Volts  	  Hz      Phase	Make	     Model		      S/no


BARUFFALDI�
TOE80�
09-11086-06�
8�
110�
50�
1�
OMRON�
3G3JV�
�
�



Computer 


	Make		Model	                    	S/no		Monitor type(if fitted)      	Dongle s/no(if fitted)


N/A�
�
�
�
�
�



Com ports	(type of socket)			        Video				Hd(cmos settings)


  Com 1	       Com 2	            Com 3	      Com 4	         card		Mem	Hdd(Mb)           Cyl	      Head	       Sec/t


�
�
�
�
�
�
�
�
�
�
�



Optional equipment


	P.chuck		Tailstock			Vice		    Air press switch		 Other


PNEUMATIC R.LEADER�
N/A�
N/A�
INPUT�
POWER DOOR�
�



Comments (include problems encountered during time in inspection)


GUARMASTER SWITCH FITTED �
�
OMRON 150(  750W RESISTOR FITTED TO ENABLE POWER LOSS BRAKING FUNCTION(ORIGINAL RESISTOR WRONG VALUE)�
�
�
�
�
�



TIMER/COUNTER/KEEPRELAY





T/C/K�
SETTING�
�
T8�
192�
�
T10�
192�
�
T28�
200�
�
C0�
2�
�
C16�
1�
�
C28�
7�
�
C36�
3�
�
K0�
00010010�
�
K1�
00010010�
�
K2�
00000011�
�
K3�
00000001�
�
K4�
00001000�
�
�
�
�



