ELECTRICAL RECORD SHEET





DATE�
MACHINE TYPE�
SERIAL NUMBER�
CUSTOMER�
�
28/05/98�
CYCLONE�
EO5415�
FESTO DIDACTIC-LAGER�
�
Inspected by:








Address-RECHBERGSTR 3, 73770 DENKENDORF�
�
GERMANY�
�
Cust order  n/o -137/45211552 �
�



Power requirements-				 		Transformer details(if supplied)


V-415�
Phase-3�
Hz-50�
V in-N/A�
V outN/A�
KVA-N/A�
�



Control system							    		 Software


 Control supplier                 Control type                 Control s/no	     	Denford-F    	    	  Denford-H	                Eprom	


FANUC�
21I - TA�
E98YAO344�
C007 D�
N/A�
�
�



Axis motors


			 Make		                   Model				  S/no		       Volts               Ac/Dc	   Phase


x-axis�
FANUC�
AO6B-0032-B075#7008�
�
176�
AC�
3�
�
y-axis�
�
�
�
�
�
�
�
z-axis�
FANUC�
AO6B-0032-B075#7008�
C98Y02074�
176�
AC�
3�
�
4th-axis�
N/A�
�
�
�
�
�
�



Axis drives


			Make		                  Model			            S/no


x-axis�
FANUC�
AO6B-6093-H111�
EA8Y50963�
�
y-axis�
�
�
�
�
z-axis�
FANUC�
AO6B-6093-H111�
EA8Y50944�
�
4th-axis�
N/A�
�
�
�



Spindle motor


	 	Make		             		Model		          			S/no			     Volts	  Hz	     Ac/Dc	Phase


KEB�
4KW�
�
420�
N/A�
AC�
3�
�



Spindle drive								  	      Spindle encoder(if fitted)


            Make		     	Model		  		 S/no			    Make			Model				  S/no	


KEB�
12.F4.C1D-3420-1.4�
98480026/0337014�
FANUC�
A680 - 0309 - T302�
�
�



Toolchanger									  	                       Invertor(if fitted)


     Make		Model		       S/no	     Stations    Volts  	  Hz	  Phase		Make		     Model		      S/no


BARUFFALDI�
TOE80�
09-10742-06�
8�
110�
50�
1�
KEB�
07.F4.SOC-M220�
99051311/0354436�
�



Computer 


	Make				       Model				S/no 				Monitor type(if fitted)		Dongle s/no(if fitted)


N/A�
�
�
�
�
�



Com ports	(type of socket)				         	         Video				Hd(cmos settings)


  Com 1	   Com 2	    Com 3	      Com 4	         card		Mem		Hdd(Mb)           Cyl		      Head	       Sec/t


�
�
�
�
�
�
�
�
�
�
�



Optional equipment


	P.chuck			Tailstock				Vice			    Air press switch			  Other


PNEUMATIC R.LEADER�
�
�
INPUT�
POWER DOOR�
�



Comments (include problems encountered during time in inspection)


GUARDMASTER�
�
�
�
�
�
�
�
�
�
TIMER/COUNTER/KEEPRELAY





�T/C/K�
SETTING�
�
T8�
192�
�
T10�
192�
�
T28�
200�
�
C0�
2�
�
C16�
1�
�
C28�
7�
�
C36�
3�
�
K0�
00010010�
�
K2�
00000011�
�
K3�
00010001�
�
K4�
00001000�
�
�
�
�
�
�
�



Spindle drive settings altered due to Op,Oc errors when 125mm chuck fitted.


op12 dec. time			=  4.50 s


Pn05 LAD load level		=  200 %


Pn06 LD voltage		=  520 V


Pn17 power off start volt	=  500 V











