DETAILS ON THE INDENTIFICATION PLATE FOR

THE DENFORD VICEROY 280 SYNCHRO LATHE 

MANUFACTURED NOVEMBER 1985

CLASSIFICATION & RATING

MODEL:      TDS/280/S

SERIAL No. 320 84/88/109

VOLTAGE:  415V   F.L.C. 3A   50 Hz     3 PH

CONTROL VOLTAGE 415 V  LIGHT VOLTAGE  12 V

MAIN MOTOR : 11/8 HP    0.82 Kw    3 PH

DATE of MANUFACTURE:  November / 1985

WIRING DIAGRAMS: A3-5000 / 14 / 15 / 16
