9pin to 9pin Test Cable
Here is the wiring on the 9to9 pin female test cable:

            1-empty                                                1-empty

                        6-white                                                  6-green

            2-blue                                                   2-brown

                        7-black                                                  7-purple

            3-brown                                                 3-blue

                        8-purple                                                 8-black

            4-green                                                 4-white

                        9-empty                                                9-empty

            5-yellow                                                5-yellow

            Shield to metal case                              Shield to metal case

The leads on pins 2 & 3 crossover



        4 & 6 crossover



        7 & 8 crossover

This cable can be used to connect the computer directly to the control card, bypassing the 25 pin connector and the inside cable on the machine.

Radio Shack Items

2 - 9-Position Female Solder D-Sub Connector 

	

	Model: 276-1538  |  Catalog #: 276-1538 


OR
 9-Position Female Crimp D-Sub Connector 
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	Model: 276-1428  |  Catalog #: 276-1428 


2 -9- and 15-Position D-Sub Connector Hood 
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	Model: 276-1539  |  Catalog #: 276-1539 


A length of 7 lead shielded cable (RS-232 cable)
