ELECTRICAL RECORD SHEET





DATE�MACHINE TYPE�SERIAL NUMBER�CUSTOMER�DATE COMMISSIONED�INITIAL��14/09/99�TRIAC VMC�EO5447/1�SANGARI����

Inspected;

Address no  SANGARI - CAMALAKIS LTD ��56 PATISSION STREET, ATHENS, 106 82, GREECE��Cust order n/o-S-C 307-3 DEN��

Power requirements-				 		Transformer details(if supplied)

V-240�Phase-1�Hz-50�V in�V out-�Kva��ontrol system								     Software

 Control supplier   	    Control type       s/no	  	    Denford-F	                   Denford-H	                   Eprom	

OPTIMISED�EUROSTEP ISS 5�0C00217096�2.102��1,.6H��

Axis motors

			 Make		                   Model				  S/no		       Volts          	Ac/Dc	   Phase

x-axis�MAE�HY200-3424-310AB��44�DC���y-axis� MAE�HY200-3424-310AB��44�DC���z-axis�MAE�HY200-3450-0350-AYOB��44�DC���4th-axis��������

Axis drives

 x-axis�DIGIPLAN�          SD12�10027233��y-axis�DIGIPLAN�          SD12�9992090��z-axis�DIGIPLAN�          SD13�10111085��4th-axis�����

Spindle motor

	 	Make		             		Model		          			S/no		   Volts	        kw	    Hz	     Ac/Dc	Phase

  SEM�MT30U4-36��140�.��DC���

Spindle drive								  	      Spindle encoder(if fitted)

            Make		     	Model		  		 S/no			    Make			Model				  S/no	

SPRINT �1200������

Toolchanger									  	                       Invertor(if fitted)

     Make		Model		       S/no	     Stations    Volts  	  Hz	  Phase		Make		     Model		      S/no

  DENFORDS�GENCAM��  8�240�50�  1�����

Computer 

	Make				       Model				S/no 				Monitor type(if fitted)		Dongle s/no(if fitted)

        GOLF�6X6-300��MICROVITEC 10”���

Com ports	(type of socket)				         Video					Hd(cmos settings)

  Com 1	   Com 2	    Com 3	      Com 4	         card		Mem		Hdd(Mb)           Cyl		      Head	       Sec/t

9 WAY�9  WAY�25 WAY��TRIDENT�32 MB�N/A�����

Optional equipment

	P.chuck			Tailstock				Vice			    Air press switch			  Other

     N/A�        N/A� N/A�N/A�N/A��

Comments (include problems encountered during time in inspection)

GUARDMASTER��POTS������

�NARROWSIMBOX 0

SHOWTOOL 0

USE3D 0

FANUC_SDEVICE machine

UTILS_MENU_1 Dos Access

UTILS_GO_1 dos

TOOLORIENT 0

HIGHSPINDLE 4000

slave_spindlef 0.85

HIGHFEED 2500

HIGHFEEDZ 1500

MAXCONTOUR 90

SLAVE_CONTOURFEED  0.15

SLAVE_CONTOURANGLE 0.15

XIO 1

nopots 0

lubesense 1

maxtool 8

moverangez 235

toolchangez 210



IBM.RS2 2

$3F8 4 COM1

$3E8 5 MACHINE

DENFORD1.KBD 1

18.2 $2F8 3

VGA.CRT 0

FANUCMD.APP


